



# TR-JB07-IN 7-inch Junction Box



## Specifications

|  |  |
| --- | --- |
| Model | TR-JB07-IN |
| Application | Outdoor or indoor cable junction box for IPC2XX and IPC32X series |
| Dimensions | 126mmx125mmx55mm (5” x4.9” x2.2”) |
| Weight | 0.72kg(1.6lb) |
| Material | Aluminium alloy |

## Dimensions

****

**Zhejiang Uniview Technologies Co.,Ltd.**

South Tower, Building 10, Wanlun Science Park, 88 Jiangling Road, Hangzhou, P.R.China 310051

Email：[overseasbusiness@uniview.com](mailto:overseasbusiness@uniview.com);globalsupport@uniview.com

http://www.uniview.com

©2015 Zhejiang Uniview Technologies Co.,Ltd. All rights reserved.

\*Product specifications and availability are subject to change without notice.